**Fixing 120 Series Toilet Partition Hardware Leg to the Floor**

**Installation Instructions**

# 120\_200SS, 120ALUM-Series, DESIGNER\_120ALUM

# Using an Allen Key, release the grub screw from the leg (Image 1).

# By completing step 1, this will release the floor grommet (Image 2).

# 

# Image 1. Image 2

# Fix grommet to the floor using screw provided.

# Return leg assembly to the base (floor grommet).

# Lock in Grub Screw using Allen Key for secure fixing.