**METLAM AUSTRALIA SHOWER SEAT CLEANING AND MAINTENANCE GUIDE**

A black and silver table

Description automatically generated

**General Cleaning**

To maintain the appearance of the shower seat surface, wipe the surface with a damp soft cloth or sponge. You may also use a mixture of warm water and mild detergent.

**After cleaning, wipe the surface with a dry soft absorbent cloth.**

**What to avoid**

* Rubbing with steel wool (wire wool) or scraping with steel tools
* Using concentrated bleach or hydrochloric acid-based cleaning products
* Abrasive cleaners
* Acidic cleaners
* Metal cleaners

**General Cleaning for stainless steel**

For everyday cleaning, wipe the surface with a damp soft cloth or sponge. You may also use a mixture of warm water and mild Neutral pH soap or detergent (such as PZ Cussons Morning Fresh).

**After cleaning, wipe the surface dry with a soft absorbent cloth.**

**Avoid Scratches**

Stainless Steel can be scratched by careless handling aggressive scrubbing. Avoid dragging rough items across the surface and be aware that grit trapped under other materials can cause surface scratches.

**Chemical Reaction**

If left in contact with salts or acids for extended periods, Metlam Australia Stainless Steel products may be compromised. Applying regular hygiene measures, like a maintenance/cleaning schedule, will minimise any potential problems.

Using incorrect cleaning products can damage your Metlam Australia stainless steel product and void the warranty.

**AVOID**

* **Rubbing with steel wool (wire wool) or scraping with steel tools.**
* **Using scourers and cleaning cloths that have been used on ordinary steel.**
* **Rubbing plastic scourers across the grain of brushed surfaces.**
* **Using concentrated bleach or hydrochloric acid-based cleaning products.**
* **Contact with products containing chlorine bleach, hydrochloric or muriatic acid.**